

*SAFEWATER* FILTER



with PATENTED SHAKE & FLUSH CLEANING PROCESS

**The perfect MSG solution for making drinking water safe!**

# Simply connect the SQUIRT to an overhead bucket for an endless supply of safe clean water

The SQUIRT-25 uses proven world class “*passive”* ultrafiltration that eliminates contaminants (pathogens, turbidity & bacteria) delivering safe, clean drinking water anywhere

# 500+

**EASY CLEAN**

L/day

**SM**&**ALL LIGHT**

#### SQUIRT *SAFEWATER* FILTER

*Meets WHO Key Drinking Water Indicators*

**Removes up to**

**99.9999**%

##### of all contaminants

Features

**Small, lightweight & portable**

##### **Easy** to use - does not require technical skills **Requires NO power** - uses gravity flow system **Removes** dirt, turbidity, pathogens, bacteria (key WHO Indicators) 0.04 Um poresize

**Quick to clean**  “SHAKE & FLUSH PROCESS” for ongoing use - does not wear out

**No chemicals added to drinking water Long life** - can be stored until needed **Designed for continuous use**

**Supplied by SkyJuice Foundation Inc.**

[www.skyjuice.org.au](http://www.skyjuice.org.au)

Tel +61 438 880 621

info@skyjuice.org.au

SQUIRT is the **perfect MSG water filtration solution** or **emergency & disaster** solution. It is Ideal for instant drinking water from dams, creeks & rivers.

## Community Use

The SQUIRT provides safe & hygienic drinking water for

remote communities, villages, schools and health clinics.

## Portable Use

The SQUIRT is lightweight and portable. You can pack

it away, store and transport the SQUIRT for use at different locations. That means clean water for IDP sites, NGO requirements, hospitals, schools, staff camps, clustered rural communities anytime, anywhere.

**NO POWER REQ’D**

**99**%

**.9999**

**REMOVAL**

**EASY TO USE**



## Setting up the Squirt -25

**SMALL**

**LIGHT**

&

**EASY CLEAN**

**500+**

L/day

### Connecting the Squirt -25

Connect the SQUIRT to an overhead water supply such as a bucket or tank. The ideal water bucket head pressure (height above water collection bucket or tank) is about 1-1.5 metres (10to 15 kPa). Output quantity will vary depending on feedwater conditions.

The maximum water head pressure should not exceed

about 3m (30 kPa). If connecting to a tank, install a

valve to turn water flow off when cleaning the unit.

**Activating the Squirt -25** (first time use only)

When using the SQUIRT for the first time flush at least 10 L of water through the SQUIRT to activate the filter fibres and remove surfactant salts. Only drink water after the first flush has been completed.

### Cleaning the Squirt -25

To maintain a good flow of drinking water the SQUIRT needs regular cleaning to remove accumulated contaminants. Undertake cleaning daily or as often as needed to maintain water flow.

#### “SHAKE & FLUSH” Cleaning Process:

1. Unclick the SQUIRT from hose.
2. Turn the SQUIRT upside down & shake vigorously until water stops flushing. If SQUIRT is extra dirty refill with water and repeat shake and flush process. Make sure to dispose dirty water to a suitable drainage area.
3. Reconnect SQUIRT to hoses and continue water filtration process.

***It is recommended*** *to undertake a monthly soak and sanitise. Use a small funnel to add a 0.2% chlorine solution to the SQUIRT-25 and allow it to soak for about 3 hours. Then undertake a “Shake & Flush” clean 3 times. This unique process removes accumulated organic and biofilm matter leading to improves flow & performance.*

### Storing the Squirt-25

When not using the SQUIRT or storing the unit for extended periods, please make sure to keep the internal filter fibres moist so they remain active. After use, drain the SQUIRT and place caps over each end to prevent evaporation before placing into safe storage at room temperature.

**ULTRAFILTRATION REMOVAL CRITERIA**

*(to 0.04um nominal)*

**ULTRAFILTRATION ULTRAFILTRATION**

**WILL REMOVE: WILL NOT REMOVE:**

PATHOGENS (disease causing CHEMICALS: including Arsenic, organisms) removed (to log reduction Cadmium, Chromium, Copper, Cyanide, value > 4) by ultrafiltration include: Fluoride, Lead, Mercury, Nickel, Nitrate,

Nitrite, Sulphate

Bacteria Total coliform TC

Protozoa Total coliform TC **MINERALS (hardness)**

Cysts Ecoli **SALINITY AND SALTS**

Helminths Virus **TOTAL DISSOLVED SOLIDS (TDS) UNPLEASANT TASTES**

**TURBIDITY (DIRT)**

**TOTAL SUSPENDED SOLIDS (TSS) IRON & MANGANESE**

*The World Health Organisation (WHO) reports that ultrafiltration provides complete removal of bacteria and viruses (disease causing pathogens) as outlined in WHO document “GUIDELINES FOR DRINKING WATER QUALITY” under “Treatment Process” as referenced in the WHO website.*

SAFEWATER FILTER

with PATENTED SHAKE & FLUSH CLEANING PROCESS

**SQUIRT-25 Specifications**

**Dimensions** 38.5cm x 6 cm dia.

**Weight** 350 grams

**Capacity** Nominal 15-25 litres/Hr

**Includes:** SQUIRT-25 WATER FILTER

+ plumbing attachment each end.

*Note: Bucket & Hose supplied separately.*

E

US

FOR Y

READ

-

TER FIL

TER A

W T

SQUIR

###### 500+

**L/day**

**Designed and manufactured in Australia**

**Supplied by SkyJuice Foundation Inc.**

[www.skyjuice.org.au](http://www.skyjuice.org.au)

Tel +61 438 880 621

info@skyjuice.org.au

****